**SLC Tray Labeling**

**Created Using:**

* **Brady BMP 51 Label Maker (use 15pt font size)**
* **Brady Cartridge MC-1500-595-WT-BK**

White Tie Wraps are to be used in the tray on the CO buffer tube

 Black Tie Wraps are to be used in the tray on the Field buffer tube

White Tape is to be used on the CO Cable

Black Tape is to be used on the Field Cable

Laminated Orange tag will be labeled with cable ID and attached to every cable at splice location

Orange wrap around tag will be attached to every cable at splice location with the arrow pointed away from C.O. (Cabinet)

NAP Tray Label Example



Mid Access Tray Label Example (Used for AF Transitions and DF Transitions and Butt Splices) Must reflect what is spliced in the tray

****

LCP Cassette Tray Label Example (Physical fiber count and port number)****

 Labeling on the LCP Door Using a P-Touch Labeler

**Outside Closure Labeling**

**Created Using:**

* **Brady BMP 51 Label Maker (use 76pt font size)**
* **Brady Cartridge MC-1500-595-ORBK**
* **3M DECAL HOLDER STRIP KIT WITH HOSE CLAMPS 3"X15" (for Medium and Large Closures)**

**** Outside Label LCP Cabinet Example

**** Medium and Large closure example using 3M Decal Holder Strip

 Aerial NAP example picture